**Crushing Hazards Inspection**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **DESCRIPTION** | | | | | | | | |
| **Date Started:** | | **/ /**  **Year Month Date** | | | | **Date Completed:** | | **/ /**  **Year Month Date** |
| **Main Purpose for the Inspection:** | |  | | | | | | |
| **Employee Name:** | |  | | | | **Checked By:** | |  |
| **Function Area:** | |  | | | | **Associated Areas:** | |  |
| **CRUSHING HAZARDS** | | | | | | | | |
| **A – Acceptable, NI – Needs Improvement, U – Unacceptable, N/A - Not Applicable** | | | | | | | | |
| **No.** | **Item Description** | | **A** | **NI** | **U** | **N/A** | **Comments** | |
| 1 | The FLHA identifies crushing hazards and control methods (e.g. body position, guarding, LOTO) | |  |  |  |  |  | |
| 2 | Controls in place to protect workers in vicinity of equipment (grinding wheels, drill presses, etc.) | |  |  |  |  |  | |
| 3 | Equipment turned off and locked out (LOTO) | |  |  |  |  |  | |
| 4 | Equipment guards in place for rotating equipment, conveyor belts, hydraulic rams, etc. | |  |  |  |  |  | |
| 5 | Hands-free zones have been identified and are known and adhered to by all personnel | |  |  |  |  |  | |
| 6 | Personnel are not in the line of fire of swinging hand tools (such as hammers) or torque tools (such as wrenches and pry bars) | |  |  |  |  |  | |
| 7 | Personnel are not in the line of fire during loading and unloading (hoisting equipment, winching, etc.) | |  |  |  |  |  | |
| 8 | Personnel PPE, hair and anything loose is secured (e.g. jewellery, hoodies), so as to not become pulled into equipment | |  |  |  |  |  | |
| 9 | Personnel wear appropriate PPE for the hazards present | |  |  |  |  |  | |
| 10 | (*add as appropriate*) | |  |  |  |  |  | |
| 11 | (*add as appropriate*) | |  |  |  |  |  | |