**Dropped Objects Inspection**

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **DESCRIPTION** | | | | | | | | | |
| **Date Started:** | | **/ /**  **Year Month Date** | | | | **Date Completed:** | | | **/ /**  **Year Month Date** |
| **Main Purpose for the Inspection:** | |  | | | | | | | |
| **Employee Name:** | |  | | | | **Checked By:** | | |  |
| **Function Area:** | |  | | | | **Associated Areas:** | | |  |
| **DROPPED OBJECTS** | | | | | | | | | |
| **A – Acceptable, NI – Needs Improvement, U – Unacceptable, N/A - Not Applicable** | | | | | | | | | |
| **No.** | **Item Description** | | **A** | **NI** | **U** | | **N/A** | **Comments** | |
| 1 | The FLHA identifies drop hazards and control methods (e.g. hoisting, lowering, working at heights) | |  |  |  | |  |  | |
| 2 | Controls are in place to protect workers below (e.g. flagging, tagging, signage, ground person, netting) | |  |  |  | |  |  | |
| 3 | Items are properly secured when manually hoisted (e.g. canvas lifting bag, proper knots) | |  |  |  | |  |  | |
| 4 | Appropriate hand tool lanyards are in use | |  |  |  | |  |  | |
| 5 | Tools and materials are properly stored so that they will not vibrate off, be knocked off, or blown off of structures | |  |  |  | |  |  | |
| 6 | Power tools are tied off during use, and cord tagged at power source. Other tools secured as required. | |  |  |  | |  |  | |
| 7 | Housekeeping in the area is maintained | |  |  |  | |  |  | |
| 8 | Small items are protected from falling through grating or off an edge (e.g. fire blanket, mesh, plywood, toe boards, etc.) | |  |  |  | |  |  | |
| 9 | Unnecessary equipment is not present (e.g. fasteners, plates, chains, piping) | |  |  |  | |  |  | |
| 10 | Area is free of ice, snow, dirt and rock build-up that could fall | |  |  |  | |  |  | |
| 11 | *(add as appropriate)* | |  |  |  | |  |  | |