Health and Safety Manual

**ABC Widget Oilfield Services Ltd. - FORMAL HAZARD ASSESSMENT**

**Task Assessed:** Operate Chop Saw

**Assessment Team:** *(needs to include affected employee)*

**FHA #:** # 006

**Revision #:** 1

John Downy; Kris Marsh; Blake Edwards

**Date:** Nov. 1, 2018

**Positions Considered:** shop & field

supers, Welders, Machinists, Labourers

**Referenced**

**Legislation:**

OH&S Code: Part

25- Tools Equipment

& Machinery

**Specialized PPE or**

**Equipment:**

Face Shield; N-95

Mask,boots,gloves,ear

muffs

Severity

Probability

1. Negligible/OK: Causing minor injury that requires first aid or

less

2. Minor: Causing non-serious injury, illness, or damage that re-

quires medical aid

3. Serious: Causing severe injury, serious illness, that is disabling

or lifelong, or property and equipment damage

4. Imminent danger: Causing death, widespread occupational ill-

ness, or loss of facilities

1. Extremely Remote: Unlikely to occur

2. Remote: Could occur at some point

3. Reasonably Probable: Likely to occur eventu-

ally

4. Probable: Likely to occur immediately or soon

Hazards

Associated with

Task

Outstanding

Implementation

Assigned To

Expected

Completion

Date

Existing Hazard Controls

Contact with

Blade

Eng: guard, adequate lighting facility

Admin: SJP # 006; Training, proper tool selection,

PPE: boots, gloves

3

3

3

4

4

4

12

12

12

3

2

2

3

3

3

9

6

6

Flying debris

(eye hazard)

Eng: guard, vacuum dust suppresion

Admin: SJP # 006, training

PPE: safety glasses

Awkward


lift/hold

Eng: integrated bench and material rest, clamp

Admin: SJP # 006, Training

PPE:

123



Health and Safety Manual

Outstanding

Implementation

Assigned To

Expected

Completion

Date

Hazards Associated

with Task

Existing Hazard Controls

Falling material (feet)

Eng: clamps

2

2

4

4

8

8

Admin: SJP # 006; Training

PPE: boots

2

2

3

3

6

6

Pinch Points

Blade failure

Eng: adequate shop lighting

Admin: SJP # 006

PPE:

Eng:

Admin: SJP # 006; pre-use inspection, PM

program, procurement Q/A

PPE:

4

2

4

4

16

8

4

2

3

3

12

6

Dust (inhalation)

Eng: vacuum dust suppression

Admin: fit testing for masks

PPE: n-95 mask

Dust

Eng: vacuum dust suppression

Admin: SJP# 006, no smoking shop policy

PPE:

Look into

automatic

sprinkler system

Jan 2019, mgmt.

team

(explosive atmosphere)

4

2

3

4

12

8

4

2

2

3

8

6


Noise

Eng:

Admin: work rotation

PPE: ear muffs

124



Only two pages were converted.

Please **Sign Up** to convert the full document.

[**www.freepdfconvert.com/membership**](https://www.freepdfconvert.com/membership)

