**Moving Objects Inspection**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **DESCRIPTION** | | | | | | | | |
| **Date Started:** | | **/ /**  **Year Month Date** | | | | **Date Completed:** | | **/ /**  **Year Month Date** |
| **Main Purpose for the Inspection:** | |  | | | | | | |
| **Employee Name:** | |  | | | | **Checked By:** | |  |
| **Function Area:** | |  | | | | **Associated Areas:** | |  |
| **MOVING OBJECTS** | | | | | | | | |
| **A – Acceptable, NI – Needs Improvement, U – Unacceptable, N/A - Not Applicable** | | | | | | | | |
| **No.** | **Item Description** | | **A** | **NI** | **U** | **N/A** | **Comments** | |
| 1 | The FLHA identifies striking hazards and control methods (e.g. body position, guarding, LOTO) | |  |  |  |  |  | |
| 2 | Controls in place to protect personnel in vicinity of moving objects | |  |  |  |  |  | |
| 3 | Exclusion zones (no-go zones) established and adhered to | |  |  |  |  |  | |
| 4 | Equipment turned off and locked out (LOTO) | |  |  |  |  |  | |
| 5 | Equipment guards in place for rotating equipment, conveyor belts, hydraulic rams | |  |  |  |  |  | |
| 6 | Personnel are using tag lines or push polls with suspended loads | |  |  |  |  |  | |
| 7 | Personnel are not in the line of fire during loading and unloading activities | |  |  |  |  |  | |
| 8 | Personnel are not in the line of fire of swinging hand tools such as hammers, etc. | |  |  |  |  |  | |
| 9 | Personnel position themselves to avoid any tension releases (stored energy) in equipment | |  |  |  |  |  | |
| 10 | *(Add as appropriate)* | |  |  |  |  |  | |
| 11 | *(Add as appropriate)* | |  |  |  |  |  | |