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Dropped Objects Inspection
	DESCRIPTION

	Date Started:
	/          /
Year      Month      Date
	Date Completed:
	/          /
Year      Month      Date

	Main Purpose for the Inspection:
	

	Employee Name:
	
	Checked By:
	

	Function Area:
	
	Associated Areas:
	

	FLHA

	A – Acceptable, NI – Needs Improvement, U – Unacceptable, N/A - Not Applicable

	No.
	Item Description
	A
	NI
	U
	N/A
	Comments

	1
	The FLHA identifies drop hazards and control methods (e.g. hoisting, lowering, working at heights)
	
	
	
	
	

	2
	Controls are in place to protect workers below (e.g. flagging, tagging, signage, ground person, netting)
	
	
	
	
	

	3
	Items are properly secured when manually hoisted (e.g. canvas lifting bag, proper knots)
	
	
	
	
	

	4
	Appropriate hand tool lanyards are in use
	
	
	
	
	

	5
	Tools and materials are properly stored so that they will not vibrate off, be knocked off, or blown off of structures
	
	
	
	
	

	6
	Power tools are tied off during use, and cord tagged at power source. Other tools secured as required.
	
	
	
	
	

	7
	Housekeeping in the area is maintained
	
	
	
	
	

	8
	Small items are protected from falling through grating or off an edge (e.g. fire blanket, mesh, plywood, toe boards, etc.)
	
	
	
	
	

	9
	Unnecessary equipment is not present (e.g. fasteners, plates, chains, piping)
	
	
	
	
	

	10
	Area is free of ice, snow, dirt and rock build-up that could fall
	
	
	
	
	

	11
	(add as appropriate)
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