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STKY Inspection Checklist
	General Information:

	Date of Inspection:
	/          /
Year      Month      Date

	Inspector Name:
	

	Location:
	

	Focus Areas

	1. Physical Hazards
☐ Unsecured heavy objects that can fall
☐ Sharp tools or machinery with exposed moving parts
☐ Unstable structures, scaffolding, or ladders
☐ Tripping hazards (cords, clutter, uneven surfaces)
☐ Confined spaces with poor ventilation
	2. Electrical Hazards
☐ Exposed or frayed wires
☐ Overloaded power strips or circuits
☐ Missing or malfunctioning grounding systems
☐ Wet conditions near electrical sources
☐ Lack of lockout/tagout (LOTO) procedures

	3. Fire & Explosion Hazards
☐ Flammable liquids/gases improperly stored
☐ Blocked or inaccessible fire exits
☐ Fire extinguishers missing, expired, or not maintained
☐ Overheated equipment or friction hazards
☐ Combustible dust buildup
	4. Chemical Hazards
☐ Toxic, corrosive, or reactive chemicals present
☐ Proper labeling and SDS (Safety Data Sheets) available
☐ Adequate ventilation and fume extraction
☐ Proper PPE (gloves, goggles, respirators) used
☐ Emergency eyewash and showers functional

	5. Biological Hazards
☐ Exposure to mold, bacteria, or viruses
☐ Presence of rodents or insects
☐ Bloodborne pathogen precautions in place
☐ Sanitation procedures followed
☐ Food and drink stored away from hazardous areas
	6. Radiation & High-Pressure Systems
☐ X-ray, laser, or radiation-emitting equipment properly shielded
☐ High-pressure gases stored securely
☐ Pressure relief valves functional
☐ Training provided for radiation or pressure system handling

	7. Vehicle & Traffic Hazards
☐ Seatbelts and safety features in working order
☐ High-visibility clothing used in work zones
☐ Forklifts and heavy machinery inspected
☐ Pedestrian walkways clearly marked
☐ Speed limits and warning signs posted
	8. Working at Heights
☐ Fall protection equipment (harnesses, guardrails) in place
☐ Roof edges and openings secured
☐ Ladders and scaffolding in good condition
☐ Safety training provided for work at heights

	9. Environmental Hazards
☐ Extreme heat/cold protection available
☐ Noise levels within safe limits (hearing protection if needed)
☐ Adequate lighting in all work areas
☐ Emergency plans in place for natural disasters
	10. Emergency Preparedness
☐ First aid kits fully stocked and accessible
☐ Emergency exits clear and properly marked
☐ Evacuation plans posted and communicated
☐ Employees trained in emergency response

	Final Notes & Observations:
____________________________________________________________________________
____________________________________________________________________________

	✔ Pass | ❌ Fail | ⚠ Needs Attention
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